/////////////////////////////////////////////////////////////////////////////
//
//Installation of the interface board device driver
//
// For Windows NT4.0(SP3)
//
//  Copyright (C) 1999 COMPUTEX CO.,LTD.
//
/////////////////////////////////////////////////////////////////////////////

1.Interface

+-----------+--------+------------------+------------+
|   Name    | Bus    |     Host         | WinNT4(SP3)|
+-----------+--------+------------------+------------+
| ISA-IF01  | ISA    | AT compatible    |     *1     |
| ISA-IF02  | ISA    | AT compatible    |     *1     |
| PCC-IF01  | PCMCIA | AT compatible    |     X      |
| PCC-IF02  | PCMCIA | AT compatible    |     X      |
| PCI-IF01  | PCI    | AT compatible    |     X      |
| PCI-IF02  | PCI    | AT compatible    |     O*2    |
+-----------+--------+------------------+------------+

    *1 See ISA_NT4.txt.
    *2 Windows NT4.0(x86) ServicePack3 or above


2.Disk content

    IF02_NT4.TXT         This file
    IF02_NT4.EXE         Installer of the WindowsNT4.0 device driver for PCI-IF02
    ISA_NT4.TXT          Description file of the WindowsNT4.0 device driver for ISA-IF01 and 02
    ISA_NT4.EXE          Installer of the WindowsNT4.0 device driver for ISA-IF01 and 02
    README.TXT           Description file of the device driver for Windows95/98/Me/2000
    CTEXW9X.INF          Interface board configuration file for Windows95/98/Me
    CTEXW2K.INF          Interface board configuration file for Windows2000
    CTEXIF02.SYS         Device driver unit for Windows2000
    CTEXIF03.SYS         Device driver unit for Windows2000
    WRTDEV0.VXD          Device driver for Windows95/98/Me
    WRTDEV1.VXD          Device driver for Windows95/98/Me
    WRTDEV2.VXD          Device driver for Windows95/98/Me
    WRTDEV3.VXD          Device driver for Windows95/98/Me
    WRTDEV4.VXD          Device driver for Windows95/98/Me
    WRTDEV5.VXD          Device driber for Windows95/98/Me
    WRTDEV6.VXD          Device driver for Windows95/98/Me
    WRTDEV7.VXD          Device driver for Windows95/98/Me
    WRTDEV8.VXD          Device driver for Windows95/98/Me
    WRTDEV9.VXD          Device driver for Windows95/98/Me


3.Installation

    For installation, log in to WindowsNT as Administrator.  Then execute IF02_NT4.EXE 
    in the CD-ROM directory (\DRIVERS) and follow instructions to set up.
    When using PCI-IF02 for the same personal computer, select by the radio button of
    IF02_NT4.EXE.  To add, re-execute IF02_NT4.EXE and select the number of board to use by
    the radio button.

    - When using one board      [1. It uses only one board.]
    - When using two boards     [2. It uses two boards.]
    - when using three boards   [3. It uses three boards.]
    - When using four boards    [4. It uses four boards.]


4.Setup of the interface board

    Log in as Administrator when installing the device driver software and changing the setting
    although CSIDE is exacutable by the user authority.


5.Version history
-------------------------------------------------------------------------
 V1.00                                                          99/05/31
-------------------------------------------------------------------------
- Initial version
