/////////////////////////////////////////////////////////////////////////////
//
//  Interface board of Computex
//  Original device driver software for WindowsNT
//
//  COMPUTEX InterfaceManager for WindowsNT(x86) Version 1.1
//
//  Copyright (C) 1997 COMPUTEX CO.,LTD.
//
//  This file explains the interface board of Computex when it is used 
//  for WindowsNT.
//
/////////////////////////////////////////////////////////////////////////////

1.The target host and interface

    IBM-PC/AT or compatible
        Must be equipped with the ISA bus
        Must be equipped with the PCI bus.  (*1)
        Must be equipped with the PC card (PCMCIA) slot.  (*1)
    Printer port
        JTAG probe to connect with the printer port.
        H-UDI probe to connect with the printer port.

     [*1]  At present, this is not available.

2.Target OS

    1)WindowsNT (x86) 3.51
    2)WindowsNT (x86) 4.0

3.Target interface

    ISA-IF01             (Interface of ISA bus)
    ISA-IF02             (Interface for ISA bus)
    PCC-IF01             (PC card [PCMCIA2.1/JEIDA4.2])(*3)
    PCC-IF02             (PC card [PCMCIA2.1/JEIDA4.2])(*3)
    PCI-IF02             (Interface for PCI bus)(*3)
    Printer port         (Probe to connect with printer port)
     [*3] At present, this is not available.

4.Software

    CSIDE95
     [Note] CSIDE (Windows3.1 for DOS) does not work for WindowsNT.

5.Contents of diskette

README.TXT        This file
SETUP.EXE         Executable file to register the driver of the interface 
                  board and to install the set up program.

6.Installation

    Log in WindowsNT with Administrator and execute SETUP.EXE. in the disk.
    After installation, the program [COMPUTEX InterfaceManager
    for WindowsNT(x86)] which is to set the device driver and 
    the interface board is registered.

7.Set up interface board

    CSIDE95 can be executed by the user but when the device driver 
    software is executed or changed, it should be logged in by Administrator.

    In order to make CSIDE95 recognize the interface board, 
    execute [COMPUTEX InterfaceManager for WindowsNT(x86)] and 
    set the type of interface board and the device address.

    Up to 8 interface boards are allowed to set by using 
    [COMPUEX InterfaceManager for WindowsNT].

[Supplement]
-------------------------------------------------------------------------
 V1.1                                                          '98/12/18
-------------------------------------------------------------------------
@ The specification addition

> It began with this version.

